


Chapter 62-701 Solid Waste Management Facilities

62-701.520 Special Waste Handling.
(1) through (5) No change.
(6) Aqueous Film-Forming Foam (AFFF) containment, collection, and disposal. AFFF as defined in Section 376.911, F.S., must be contained, collected, and disposed pursuant to the following requirements.
(a) Container management. General requirements for the storage of AFFF.
1. AFFF containers must be:
a. Clearly labeled with the words “AFFF”,
b. In good condition (no rusting, structural defects or deterioration), and
c. Not leaking (there are no visible leaks).
2. No later than 180 days after [effective date of rule], all entities storing AFFF containers must satisfy at least one of the following requirements: 
a. The AFFF container must be closed and stored inside a building with an impervious floor; or 
b. If the AFFF container is exposed to the elements, the container must be closed and inside a protective weatherproof cabinet, box, or cover on a concrete slab and must have secondary containment that has the capacity to hold 110 percent of the volume of the largest container within the containment area. 
The requirements of this subparagraph do not apply to stationary storage tanks, hard piping, or distribution systems that store or distribute AFFF. 
AFFF containers must be closed and stored inside a building with an impervious floor or, if exposed to the elements, the container must be closed and inside a protective weatherproof cabinet, box, or cover on a concrete slab and must have secondary containment which has the capacity to hold 110 percent of the volume of the largest container within the containment area.
(b) Collection and transportation. AFFF must be collected and transported by a transporter authorized to transport manifested waste pursuant to Rule 62-730.170, F.A.C.
(c) Disposal. AFFF must be disposed at permitted facilities authorized for AFFF disposal or transferred out of state for lawful use. Effective July 1, 2027, a disposal plan of remaining inventories of AFFF must be submitted to the department pursuant to s. 376.911(3)(b), F.S. The disposal plan must specify the following:
1. The transporter authorized under paragraph 62-701.520(6)(b), F.A.C., that will collect and transport the AFFF; 
2. The amount of AFFF to be collected and transported; 
3. The timeline for collection and transport of AFFF; and 
4. The authorized facility that will accept the AFFF for disposal or the out of state location where the AFFF will be transferred to for lawful use, and specify which registered Hazardous Waste (HW) transporter will collect/transport the AFFF and at what permitted disposal facility the AFFF will be disposed and when. 
If For any amount of AFFF inventory will not be being disposed or transferred cite the applicable, the disposal plan must identify the amount not being disposed, and detail which exclusion under s. 376.911(5), F.S., applies, and provide an explanation how the planned continued possession or use satisfies the cited exclusion. how the planned use meets the exclusion. Disposal plans must be submitted to AFFFInventory@FloridaDEP.gov, or to the Department of Environmental Protection, Solid Waste Section, MS 4565, 2600 Blair Stone Road, Tallahassee, Florida 32399-2400.
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