## Section B.7: “Low Yield/Poor Quality” Cleanup Target Levels

The use of Low Yield/Poor Quality criteria (see subsections 62-780.200(28) and (39), F.A.C.) is allowable under RMO II and RMO III (subsections 62-780.680(2) & (3), F.A.C.) provided a determination has been made by FDEP that it is appropriate for the site. Guidance for the evaluation of low yield/poor quality criteria can be found on FDEP’s website at: <https://floridadep.gov/waste/district-business-support/content/waste-cleanup-program-guidance>.

If the responsible party has been approved by FDEP to utilize the low yield/poor quality cleanup target levels (CTLs) for groundwater and corresponding leachability-based CTLs for soil, then the IC should identify the property as having low yield/poor quality groundwater, and it should prohibit the use of groundwater on the property. The restriction on the use of groundwater is required because contaminants will be allowed to remain at higher levels than the default health-based CTLs based on a determination that the groundwater already is of low yield or poor quality.