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This permit is issued under Section 403.0885, Florida Statutes (F.S.), and implemented through applicable provisions of Chapter 62-4, Chapter 62-620, and Chapter 62-621, Florida Administrative Code (F.A.C.). Coverage under this generic permit constitutes authorization to discharge stormwater from construction activities to surface waters of the state pursuant to the Department of Environmental Protection’s (Department, DEP) federally approved National Pollutant Discharge Elimination System (NPDES) stormwater program. This generic permit, herein referred to as the Construction Generic Permit (CGP), is adopted and incorporated by reference in paragraph 62-621.300(4)(a), F.A.C.
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[bookmark: _Toc210027249]1	PERMIT COVERAGE
[bookmark: _Toc210027250]1.1	ELIGIBILITY CONDITIONS
1.1.2	An NPDES stormwater construction generic permit (CGP) is required for large and small construction activities that are not located on Indian Lands (NPDES coverage on Indian Lands is issued by the U.S. Environmental Protection Agency) and:
a.	Will disturb one or more acres of land, or disturbs less than one acre of land but are part of a common plan of development or sale that will ultimately disturb one or more acres of land; and
b.	Discharge, or have the potential to discharge, stormwater to surface waters of the state or through a Municipal Separate Storm Sewer System (MS4); or
c.	Are designated by DEP or EPA as needing permit coverage under 40 CFR § 122.26(b)(15)(ii).
[bookmark: _Hlk138954237]1.1.3	For activities that meet the criteria in Part 1.1.2, you, the operator, are responsible for obtaining permit coverage.
1.1.4	If a contractor or subcontractor is acting under the direction of an operator that has received coverage under the CGP,  the contractor or subcontractors do not have to obtain separate coverage under this permit, but must be named on the operator’s Stormwater Pollution Prevention Plan (SWPPP) and separately sign the SWPPP certification (Part 6.1.1). 
All operators, acting independently, must obtain permit coverage. All operators of construction activity that meets the eligibility conditions in Part 1.1 shall either obtain coverage under this CGP or under an individual stormwater permit. Coverage under an individual stormwater permit may be obtained by contacting the appropriate DEP district permitting office.
1.1.5	Coverage under this permit may be suspended, revoked, or terminated in accordance with Rule 62-620.345, F.A.C., if the Department determines that there has been a violation of any terms or conditions of the permit, there has been a violation of surface water quality standards, or the operator has submitted false, incomplete or inaccurate information. 
[bookmark: _Toc210027251]1.2	GENERAL EFFLUENT LIMITATION
In the absence of information demonstrating otherwise, DEP expects that compliance with the requirements of this permit results in stormwater discharges controlled as necessary to meet surface water quality standards. If at any time you become aware of, or DEP determines that, discharges are not being controlled as necessary to meet surface water quality standards, you must take corrective action as required in Part 4.
DEP may require additional stormwater controls or revoke coverage and require you to obtain coverage under an individual stormwater permit if DEP determines that your discharges are not controlled as necessary to meet surface water quality standards.
[bookmark: _Toc210027252]1.3	AUTHORIZED DISCHARGES
1.3.1	This permit authorizes the following types of stormwater discharges to surface waters of the state or through an MS4, provided that appropriate stormwater controls are designed, installed, and maintained:
a.	Stormwater discharges, including stormwater runoff and surface runoff and drainage, associated with construction activity, as defined in 40 CFR § 122.26(b)(14)(x) or § 122.26(b)(15)(i);
b.	Stormwater discharges from an on or off-site construction support activity provided that:
i.	It is directly related to a construction site covered by this permit;
ii.	It is not a commercial operation;
iii.	It does not serve multiple unrelated construction sites; and
iv.	Stormwater controls are implemented in accordance with Part 2.
1.3.2	The following types of non-stormwater discharges are authorized provided they do not cause or contribute to a violation of surface water quality standards:
a.	Discharges from emergency firefighting activities;
b.	Fire hydrant flushing;
c.	Water used to wash vehicles and equipment, provided that there is no discharge of soaps, solvents, or detergents used for such purposes;
d.	Waters used to control dust;
e.	Potable water such as uncontaminated water line flushing;
f.	Landscape irrigation water and drainage;
g.	External building washdown provided that there is no discharge of soaps, solvents, and detergents used for such purposes, and external surfaces do not contain hazardous substances;
h.	Pavement wash waters, provided that there is no discharge of soaps, solvents, and detergents used for such purposes, and they do not contain toxic or hazardous materials from leaks or spills;
i.	Uncontaminated air conditioning or compressor condensate;
j.	Uncontaminated ground water or spring water;
k.	Foundation or footing drains where flows are not contaminated;
l.	Uncontaminated dewatering water discharged in accordance with Parts 1.3.3 and 2.4; and
m.	Discharges of stormwater covered under another NPDES permit.
1.3.3	Discharges from Dewatering. This permit may authorize the discharge of uncontaminated groundwater. The operator may obtain authorization to discharge uncontaminated ground water resulting from construction-related dewatering operations under this permit. To obtain this authorization, you must:
a.	Ensure that discharges from dewatering operations will not be contaminated. Confirm that either:
i.	the dewatering site is not identified as contaminated (contains or did contain pollutants of concern in the groundwater that exceed the surface water criteria in 62-302.530, F.A.C.) and there is no identified contaminated area within 500 feet, or
ii. 	the dewatering site is identified as contaminated or within 500 feet of a contaminated area, and 
(1) you have obtained documentation from DEP that confirms the contamination has been remediated; or 
(2) you have obtained sampling data that confirms that no pollutants of concern are present in groundwater in concentrations equal to or greater than the surface water criteria in Rule 62-302.530, F.A.C.
b.	Complete Part VI of the Notice of Intent (NOI); and
c.	Identify in the SWPPP (Part 6) and implement appropriate dewatering Best Management Practices (BMPs) (Part 2.4) to ensure that discharges from dewatering operations do not cause or contribute to violations of surface water quality standards.
[bookmark: _Toc210027253]1.4	PROHIBITED DISCHARGES.
1.4.1	Non-stormwater discharges not listed in Part 1.3.2 are prohibited, including but not limited to: 
a.	Wastewater from concrete washout;
b.	Wastewater from washout of stucco, paint, form release oils, curing compounds, and similar materials;
c.	Fuels, oils, or other pollutants used in vehicle and equipment operation and maintenance;
d.	Soaps, detergents, solvents, or other cleaners;
e.	Hazardous or toxic substances, or oil resulting from a spill or other release;
f.	Solid materials, including building materials, debris, and trash; and
g.	Any other non-stormwater discharge not authorized in Part 1.3.
1.4.2	You are prohibited from hosing down or sweeping soil or sediment accumulated on impervious surfaces into receiving waters or MS4s, or into natural or constructed drainage features or storm drain inlets, unless those features or inlets are connected to an on-site sediment basin, sediment trap, or similar control.
[bookmark: _Toc210027254]1.5	LIMITATIONS OF COVERAGE
This permit does not authorize discharges that:
1.5.1	Cause or contribute to a violation of surface water quality standards, or discharges that DEP determines to, or may reasonably be expected to, cause or contribute to a violation of surface water quality standards; 
1.5.2	Are mixed with non-stormwater, except as otherwise provided in Part 1.3.2;
1.5.3	Are associated with construction activities that have existing coverage under an individual permit.
1.5.4	Dewatering discharges that do not meet the conditions in Part 1.3.3. If dewatering discharges do not meet the conditions in Part 1.3.3, the operator shall cease those dewatering operations under this permit. Those discharges may qualify for coverage under Generic Permit for Discharge of Ground Water from Dewatering Operations (subsection 62-621.300(2), F.A.C.), or under an individual wastewater permit on the appropriate form listed in Rule 62-620.910, F.A.C.
[bookmark: _Toc210027255]1.6	ADMINISTRATIVE PROCESS FOR OBTAINING COVERAGE 
Operators who are seeking coverage under this permit must submit to the Department a complete and accurate “Notice of Intent for NPDES Construction Generic Permit, DEP Form 62-621.300(4)(b),” (NOI) and associated fee as listed in 62-4.050(4)(d)(1), F.A.C. You must develop and be ready to implement a SWPPP prior to submitting your NOI.
1.6.1	Submitting the Notice of Intent (NOI). 
You must submit your NOI and payment electronically through the DEP electronic submission portal in accordance with paragraph 62-620.100(3)(bb), F.A.C.
1.6.2	Signatory requirements. The responsible authority as described in subsection 62-620.305(1), F.A.C., must sign the NOI.
Duly Authorized Representative. The responsible authority may designate a duly authorized representative in accordance with subsection 62-620.305(2), F.A.C., by submitting signed documentation to the Department.
1.6.3	Deadlines for Submitting the NOI. For a new project, you must submit a complete NOI and permit fee at least 2 calendar days before the commencement of construction activities.
To renew coverage for a project continuing beyond the five-year term of existing CGP coverage, you must submit the complete NOI and permit fee at least 2 calendar days before your current permit coverage expires.
For a project where the operator changes, the new operator must submit a complete NOI and permit fee at least 2 calendar days before assuming control of the project. 
When the complete NOI is received, the Department will send you an acknowledgment letter that will identify the permit number, term of permit coverage and a copy of the CGP. 
If the project discharges stormwater to an MS4, you must send a copy of the NOI and acknowledgement letter to the MS4 operator(s) within 7 calendar days of receipt of the acknowledgement letter.
1.6.4	Term of Permit Coverage. The term of your permit coverage begins the day after the Department sends an acknowledgement letter and expires after five years. Once covered under this permit, your coverage will be valid until the date that either:
a. 	You terminate permit coverage (Part 7), 
b. 	You renew permit coverage, 
c. 	DEP terminates coverage, or
d.	Permit coverage expires.
1.6.5	Waivers from electronic submission. Waivers may be granted based on either (1) your operational headquarters is located in a geographic area that is identified as under-served for broadband internet access in the most recent report from the Federal Communications Commission, or, (2) you have limitations regarding available computer access/computer capability.
If DEP grants approval, you must complete a paper NOI that can be obtained by mailing a request to NPDES Stormwater Notice Center, 2600 Blair Stone Rd., MS 3585, Tallahassee, FL 32399, and submit a completed paper NOI, along with your permit fee, to Florida Department of Environmental Protection, PO Box 3070, Tallahassee, FL 32315.
1.6.6	Coverage under this permit is not transferrable to new operators or new sites/projects. If there is a change of operators, the current operator must submit an NOT in accordance with Part 7 and the new operator must submit an NOI in accordance with Part 1.

1.6.7	Updating operator information. If you need to correct or update any operator information after submitting the NOI, you may do so using the DEP electronic submission portal.

1.6.8	Modifications to construction activities or site information. If construction activities change, you must submit a request to modify the coverage by using the DEP electronic submission portal.

In accordance with paragraph 62-4.050(4)(s), F.A.C., a processing fee may apply for minor technical changes that involve new activities.

Until notified by DEP, you may continue to operate based on the information provided in your original NOI, but you must wait until a revised acknowledgment letter is received before you commence activities on any portion of your site that would be affected by any modifications. 
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1.7	PUBLIC NOTICE OF PERMIT COVERAGE.
You must post a notice of permit coverage at a safe, publicly accessible location in close proximity to the construction activity to include:
a.	A copy of the NOI or acknowledgment letter; and
[bookmark: _Hlk207006792]b.	The following statement: “If you observe erosion, polluted runoff, or stormwater pollution from this construction site, contact the appropriate Florida Department of Environmental Protection District Office at https://floridadep.gov/districts.”
[bookmark: _Toc210027257]2	STORMWATER CONTROL REQUIREMENTS
[bookmark: _Toc210027258]2.1	GENERAL REQUIREMENTS
You must design, install, and maintain appropriate stormwater controls to minimize the discharge of pollutants in stormwater from construction activities. 
2.1.1	Design and install all stormwater controls in accordance with applicable requirements and consistent with the guidelines contained in the State of Florida Erosion and Sediment Control Designer and Reviewer Manual, FDOT and DEP (2013) (http://www.flrules.org/Gateway/reference.asp?No=Ref-04227).
2.1.2	Install perimeter controls before commencement of construction activities and prior to earth-disturbing activities in each phase of construction (minimize exposed soil during the initial installation of perimeter controls).
2.1.3	Ensure all stormwater controls are maintained and remain in effective operating condition and are protected from activities that would reduce their effectiveness. Adhere to applicable manufacturer’s maintenance recommendations. Maintenance that is required to ensure a stormwater control meets the conditions of this permit shall be completed within 7 calendar days following discovery.
2.1.4	Identify contingencies in the SWPPP to implement in order to minimize impacts from stormwater discharges during major storm and flooding events such as tropical depressions, tropical storms, hurricanes, storm surge, and extreme rainfall.
[bookmark: _Toc210027259]2.2	EROSION AND SEDIMENT CONTROL REQUIREMENTS
Implement erosion and sediment controls to minimize the discharge of pollutants in stormwater from construction activities. In selecting erosion and sedimentation controls, you must consider factors such as the amount, frequency, intensity, and duration of precipitation, characteristics of resulting stormwater, topography, and site soil characteristics, including the range of soil particle sizes expected to be present.
2.2.1	Install controls along any perimeters of the site that are downgradient of exposed soil or other disturbed areas.
a.	Perimeter controls must be installed upgradient of natural buffers designated under Part 2.2.2a.;
b.	After installation of perimeter controls, remove sediment before it has accumulated to one-half of the above-ground height to maintain effective operating condition.
2.2.2	Designate and maintain existing vegetated areas to serve as natural buffers between construction activity and receiving waterbodies. If any portion of the site’s earth disturbing activities are located within 50 feet of a waterbody, and those portions discharge stormwater to that waterbody, you must comply with one of the following for those portions of the site:
a.	Designate and maintain a 50-foot undisturbed natural buffer downgradient of perimeter controls; or
b.	If a 50-foot natural buffer is not designated, supplement the perimeter control with additional perimeter controls; or
c.	Implement controls to capture or divert stormwater flows from those portions of the site.
2.2.3	Direct stormwater to vegetated areas and maximize stormwater infiltration and filtering, unless not technologically possible or not economically practicable and achievable in light of best industry practices.
2.2.4	Minimize off-site sediment track-out at vehicle access points.
a.	Restrict use to properly designated access points;
b.	Implement and maintain tracking prevention controls, as necessary, to ensure sediment removal occurs prior to vehicle exit; and 
c.	Remove off-site accumulation of sediment due to vehicle track-out by the end of the same business day that it was identified.
2.2.5	Minimize the amount of soil exposed or disturbed during construction activities.
2.2.6	Manage stockpiles or land clearing debris piles:
a.	Locate stockpiles away from natural buffers and away from constructed or natural site drainage features, storm drain inlets, and areas where stormwater flow is concentrated;
b.	Install a sediment barrier along all downgradient perimeters of stockpiled soil or land clearing debris piles;
c.	For piles that will be unused for 7 or more days, provide cover or appropriate temporary stabilization.
2.2.7	Minimize dust with the appropriate application of water or other appropriate BMPs.
2.2.8	Preserve and reapply native topsoil, where feasible.
2.2.9	Minimize soil compaction. Restrict vehicle/equipment use in areas of your site where final stabilization will occur or where infiltration practices will be installed.
[bookmark: _Hlk205984824]2.2.10	Protect storm drain inlets.
a.	Install and maintain inlet protection measures designed to remove sediment from stormwater discharges prior to entry into any stormwater conveyance that carries stormwater from your site. Inlet protection measures are not required for storm drain inlets that are not yet connected to the final drainage network, still under construction, or conveyed to an onsite sediment basin, sediment trap, or similar control; and
[bookmark: _Hlk192678365]b.	Clean or replace inlet protection measures as sediment accumulates and/or performance is compromised; inlet protection measures may be removed in the event of flood conditions.
[bookmark: _Hlk205985025]2.2.11	Control stormwater volume and velocity within the site to minimize on-site soil erosion and offsite sedimentation, and to minimize the discharge of pollutants.
2.2.12	Control stormwater discharge rates at the discharge points to minimize erosion at outfalls and to minimize downstream channel erosion, streambank erosion, and scouring.
2.2.13	For sites with 10 or more acres disturbed at one time (whether contiguous or throughout the project site), the following conditions shall be met until final stabilization of the disturbed area is achieved:
a.	Design, install, and maintain a temporary sediment basin, or a combination of sediment basins, sediment traps, or other BMPs, to provide storage for 3,600 cubic feet per acre drained; this does not apply to flows from off-site areas and flows from on-site areas that are either undisturbed or have undergone final stabilization where such flows are diverted around both the disturbed area and the sediment basin.
b.	Areas that will be used for permanent stormwater infiltration treatment (e.g., stormwater retention basins) should not be used for temporary sediment basins unless appropriate measures are taken to remove accumulated fine sediments, avoid excessive compaction of soils by construction machinery or equipment, and ensure that the design infiltration capacity is met at final stabilization;
c.	Situate the basin outside of any receiving water and any designated natural buffers;
	d.	Remove accumulated sediment to maintain at least one-half of the design capacity and conduct all other appropriate maintenance to ensure the basin or impoundment remains in effective operating condition.
2.2.14	Stabilize exposed portions of the site. Implement and maintain vegetative or non-vegetative stabilization measures that minimize erosion from areas of exposed soil on the site.
You must initiate permanent or temporary stabilization measures within 7 calendar days after construction activities have ceased for any portion of the site.
[bookmark: _Toc210027260]2.3	POLLUTION PREVENTION REQUIREMENTS
You must install and maintain pollution prevention control BMPs to minimize the discharge of pollutants in stormwater and to prevent the discharge of pollutants from spills or leaked materials from construction activities.
2.3.1	Establish a spill prevention and response plan to safely eliminate and clean up any spilled or leaked chemicals, including fuels and oils.
a.	Comply with applicable federal and state requirements regarding the storage of chemicals;
b.	Clean up spills immediately using dry clean-up methods where possible; dispose of used materials according to state regulations;
c.	Ensure adequate supplies are available at all times to handle spills, leaks, and disposal of used liquids;
d.	Use drip pans and absorbents where appropriate.
e.	Contact information (e.g. notification chain) for appropriate personnel and/or spill response entities must be in locations that are readily accessible to all persons identified in the SWPPP in the event of a spill.
2.3.2	Emergency Spill / Hazardous Release Notification Requirements. 
Pursuant to 403.077, F.S., an owner or operator of the installation at which the reportable pollution release occurred must provide to the Department information reported to the SWO within 24 hours of the owner’s or operator’s discovery of such reportable pollution release. This shall be provided using the Public Notice of Pollution website at https://floridadep.gov/pollutionnotice.
Notify the State Watch Office (SWO) (800-320-0519 or 850-815-4001) as soon as you have knowledge of the discharge.
2.3.3	Implement BMPs to minimize the discharge of pollutants from equipment and vehicle rinsing and washing.
2.3.4	Storage, handling, and disposal of building products, materials, chemicals, and wastes. 
a.	Provide either cover (e.g., plastic sheeting, temporary roofs, covered containers) or a similarly effective means to minimize the exposure of the following products to precipitation and stormwater runoff: 
i.	paints, concrete, and stucco;
ii.	soaps, detergents, or solvents;
ii.	pesticides, herbicides, and fertilizers;
iv.	building materials, building products (minimization of exposure to stormwater is not required where the material or product poses little risk of stormwater contamination). 
b.	Follow all federal and state requirements regarding storage of petroleum products.
c.	Follow all federal and state requirements regarding disposal of construction, solid, hazardous or toxic waste.
d.	Provide and maintain waste containers of sufficient size and number to contain wastes generated onsite; position waste containers near active construction.
e.	Position portable toilets so they are secure and will not be tipped or knocked over, and are located away from receiving waters, storm drain inlets and constructed or natural site drainage features.
2.3.5	Washing containers and applicators used for stucco, paint, concrete, form release oils, curing compounds, or other materials:
a.	Designate and physically label (e.g. with signage) areas for washwater;
b.	Direct washwater to a container, lined pit, or similarly effective control;
c.	Conduct washout activities in areas that are designated and labeled; do not allow liquid wastes to be disposed of on the ground; 
d.	To the extent feasible, locate washout areas near active construction and away from receiving waters, constructed or natural drainage features, and storm drain inlets.
e.	Comply with applicable federal or state requirements for disposal of washwater wastes.
[bookmark: _Toc210027261]2.4	DEWATERING REQUIREMENTS
The requirements of this section apply to construction site dewatering operations, in accordance with Part 1.3.3, that are otherwise not covered by another NPDES permit such as the Generic Permit for Discharge of Ground Water from Dewatering Operations (subsection 62-621.300(2), F.A.C.).
2.4.1	Implement appropriate BMPs that are consistent with the State of Florida Erosion and Sediment Control Designer and Reviewer Manual, FDOT and DEP (2013);
2.4.2	Route dewatering water through a sediment control (e.g. vegetated swale, sediment trap, filter bag) and use stable, erosion-resistant surfaces (e.g. clean filter stone, geotextile underlayment);
2.4.3	To the extent feasible, discharge dewatering water onto vegetated upland areas of the site where the water can infiltrate or into the permitted stormwater system serving the project site.
2.4.4	Properly dispose of backwash water or return to the beginning of the treatment process.
2.4.5	Inspect dewatering discharges from points of discharge to receiving waterbodies or MS4s at least once per day while discharging.
[bookmark: _Hlk153368513]a.	Inspect for a sediment plume, unusual color, presence of odor, decreased clarity, presence of foam, a visible sheen on the water surface or visible oily deposits in receiving waters or MS4; initiate corrective action, as required.
b.	Record/log the following at the time of inspection:
i.	The inspection date;
ii.	Names and titles of personnel conducting the inspection;
iii.	A summary of inspection findings and observations.
[bookmark: _Toc210027262][bookmark: _Hlk196827491]2.4.6	TURBIDITY BENCHMARK MONITORING
The requirements of this section apply to sites conducting dewatering operations with direct discharges to waters of the state that are designated as Outstanding Florida Waters (OFW) or verified by DEP as impaired for sediment or a sediment-related parameter. Waters verified by DEP as impaired for sediment, or a sediment-related parameter, can be found at  https://floridadep.gov/dear/water-quality-restoration/content/impaired-waters-tmdls-and-basin-management-action-plans; OFWs are identified in subsection 62-302.700(9), F.A.C. Turbidity benchmark monitoring, and the noted threshold, is intended to serve as an indicator of the effectiveness of dewatering controls; the benchmark threshold is not an effluent limitation.
[bookmark: _Hlk205985199]a.	Turbidity monitoring requirements
i.	Sampling location. You must take samples at the point(s) of discharge to receiving waters after the dewatering water has been routed through any sediment controls and/or treatment devices. Background samples must be taken upstream from the discharge point, or in an area absent of the dewatering discharge.
ii.	Sampling frequency. You must collect at least one turbidity sample from your dewatering discharge to receiving waters and one sample upstream of the discharge point each day a discharge occurs. 
iii.	Monitoring week. For the purpose of calculating averages, the monitoring week starts on Monday and ends on Sunday. Once a new monitoring week starts, you will need to calculate a new average for that week of monitoring results. A weekly average shall consist of one or more monitoring results.
iv.	Test methods. You must measure samples using a turbidity meter that reports results in nephelometric turbidity units (NTUs). You must conduct a calibration verification in accordance with the manufacturer’s instructions prior to each day’s use.
[bookmark: _Hlk205985235]	b.	Turbidity benchmark. The benchmark threshold for turbidity for this permit is:
i.	0 NTUs above the monitoring week average background conditions for waters designated as OFWs; or
ii.	29 NTUs above the monitoring week average background conditions for waters, other than OFWs, verified as impaired by DEP for sediment or a sediment-related parameter.
	c.	Comparison of turbidity samples to benchmark. Compare the weekly average of your turbidity monitoring results to the applicable benchmark.
i.	All samples taken in accordance with Part 2.5.1d shall be used to calculate your weekly average.
ii.	If you are conducting turbidity monitoring for more than one dewatering discharge point, you must calculate a weekly average turbidity value for each discharge point and compare each to the turbidity benchmark.
2.5.4	If the weekly average of your turbidity monitoring results exceeds the applicable benchmark threshold, you must take corrective action to address the exceedance; corrective action must be completed within 7 calendar days.
2.5.5	Recordkeeping. You must maintain records of individual sampling dates and results, the weekly average benchmark and turbidity results, calibration verification, and any corrective action taken to address exceedances of applicable benchmark thresholds. You must retain all monitoring information for three years from the date that the site has reached final stabilization and the Notice of Termination (NOT) has been submitted.
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[bookmark: _Toc210027264]3.1	INSPECTOR REQUIREMENTS
Inspections conducted pursuant to this Part shall be conducted by a qualified inspector (see Part 5.3). The person(s) inspecting your site may be a person employed or under contract by you. 
[bookmark: _Toc210027265]3.2	INSPECTION FREQUENCIES
3.2.1	Your site must be inspected within seven calendar days of the last inspection, or by the end of the next working day following the end of a storm event that is 0.50 inches or greater, whichever comes first. The first inspection must occur within seven calendar days of commencement of construction activities.
3.2.2	To determine whether a storm event requires an inspection under Part 3.2.1, you must either keep a functional rain gauge on your site or obtain rainfall data from a weather station that is representative of your location.
[bookmark: _Toc210027266]3.3	REDUCTIONS IN INSPECTION FREQUENCIES
3.3.1	For areas where you have achieved final stabilization, you may suspend inspections.
3.3.2	For areas where you have achieved temporary stabilization, you may reduce the frequency of inspections to once per month, provided:
a.	The temporary stabilization measures are successful at stabilizing the site for the duration of your suspended construction activities; and 
b.	You have updated the SWPPP to include:
i.	The status and type of stabilization implemented, 
ii.	The date the activities were suspended, and
iii.	The projected date activities will resume. 
If construction activity resumes in this portion of the site at a later date, the inspection frequency immediately returns to the inspection frequency in Part 3.2.1. You are at all times responsible for ensuring that your stabilization methods are in effective operating condition and in compliance with permit requirements. 
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Your qualified inspector must inspect all stormwater, erosion, sedimentation, and pollution prevention controls used at the site to comply with this permit.
3.4.1	The following areas of your site must be inspected, as applicable (you are not required to inspect areas that, at the time of the inspection, are considered unsafe to inspection personnel):
a.	All areas that have been cleared, graded, or excavated and have not completed stabilization consistent with Part 2.2.16;
b.	Material, waste, borrow, and equipment storage and maintenance areas;
c.	All areas where stormwater typically flows within the site, including constructed or natural site drainage features designed to divert, convey, and/or treat stormwater;
d.	All areas where construction dewatering is taking place, including controls to treat the dewatering discharge and any channelized flow of water to and from those controls;
e.	Inspect all discharge points from the site to ensure stormwater discharges are not resulting in offsite sedimentation or causing or contributing to violations of surface water quality standards;
f.	All locations where temporary stabilization measures have been implemented;
g.	All locations where vehicles enter or exit the site for evidence of offsite sediment tracking.
3.4.2	During each site inspection, your qualified inspector must at a minimum:
a.	Inspect all erosion, sedimentation, and pollution prevention controls to ensure that they are installed, maintained, and operating correctly and effectively;
b.	Check for indicators of spill, leaks, or other accumulations of pollutants on the site, or the presence of conditions that could lead to their occurrence;
c.	Check for signs of visible erosion and sedimentation that have occurred and are attributable to discharges from your site at discharge point(s) and, if applicable, on the banks/bottom of any receiving waters or MS4 flowing within or immediately adjacent to the site;
d.	Check for signs of sediment deposition and other pollutants that are visible from your site and attributable to discharges from your site, including within receiving waters and MS4s;
e.	Identify any incidents of noncompliance observed; and
f.	If a discharge from the construction site is occurring during your inspection, observe and document the visual quality of the discharge. Document the characteristics of the stormwater discharge including color, odor, any floating, settled, or suspended solids, and any foam, oil sheen, and other indicators of stormwater pollutants. 
3.4.3	Based on the results of inspections, you must:
a.	Identify any locations where new or modified controls are necessary to meet permit requirements; and
b.	Initiate any necessary maintenance repairs, replacements, or corrective action.
[bookmark: _Toc210027268]3.5	INSPECTION FORMS AND RECORDKEEPING
3.5.1	Your inspector must complete and sign an inspection report within 24 hours of conducting an inspection. Each report shall include the following:
a.	Permit number;
b.	Date of the inspection;
c.	Name and title of qualified personnel conducting the inspection;
[bookmark: _Hlk153368803]d.	A summary of inspection findings, including documentation of routine maintenance including replacement and/or repairs, and observations that initiate corrective action;
e.	If triggered by a storm event, include the rain gauge or weather station readings; and
f.	If you determined that it is unsafe to inspect a portion of your site, describe the circumstances and locations to which this condition applies.
3.5.3	You must maintain copies of all inspection reports at the site or an easily accessible location, to include electronic recordkeeping systems, so they can be made available at the time of an inspection or upon request  in accordance with Rule 62-621.260, F.A.C.
3.5.4	Keep inspection records for three years from the date that the NOT is submitted or coverage expires.
[bookmark: _Toc210027269]4	CORRECTIVE ACTION

If it is discovered that a stormwater control was not installed/implemented or needs replacement, or if a prohibited discharge is observed, you must immediately take all reasonable steps to address the condition and complete any corrective action within 7 calendar days.

[bookmark: _Toc210027270]4.1	CONDITIONS TRIGGERING CORRECTIVE ACTION
You must take corrective action to address any of the following conditions identified at your site:
4.1.1	A stormwater control necessary to comply with the requirements of this permit was never installed, or was installed incorrectly; or
4.1.2	Your discharges are not meeting surface water quality standards; or
4.1.3	A prohibited discharge has occurred; or
4.1.4	If conducting dewatering operations you observe or are informed of the presence of:
a.	a sediment plume, suspended solids,
b.	unusual color, presence of odor, decreased clarity, or presence of foam; and/or
c.	a visible sheen on the water surface or visible oily deposits on the bottom or shoreline of the receiving water or MS4.
[bookmark: _Toc210027271]4.2	CORRECTIVE ACTION REQUIRED BY DEP OR EPA
You must comply with any corrective actions required by EPA or DEP as a result of permit violations found during an inspection.
[bookmark: _Toc210027272]4.3	CORRECTIVE ACTION RECORDKEEPING
4.3.1	Within 24 hours of identifying a condition requiring corrective action, you must document the specific condition and the date and time it was identified.
4.3.2	You must document completion of corrective action on the subsequent inspection report/form.
4.3.3	Each record of corrective action must be signed by a responsible authority or a duly authorized representative in accordance with Rule 62-620.305, F.A.C.
4.3.4	You must keep copies of all corrective action records with the SWPPP.
4.3.5	Any corrective action that results in changes to any permit-required controls or site conditions must be reflected in the SWPPP within seven calendar days of completing the corrective action.
[bookmark: _Toc210027273]5	PERSONNEL RESPONSIBILITIES AND TRAINING REQUIREMENTS
[bookmark: _Toc210027274]5.1	STORMWATER TEAM
You must assemble a stormwater team that will be responsible for carrying out activities necessary to comply with this permit. The stormwater team must be identified in the SWPPP and consist of personnel who are responsible for:
a.	the design, installation, maintenance, and/or repair of stormwater erosion, sedimentation and pollution prevention controls;
b.	conducting inspections;
c.	ensuring corrective actions are completed.
[bookmark: _Toc210027275]5.2	GENERAL TRAINING REQUIREMENTS
Prior to the commencement of construction activities, you must ensure that all members of the stormwater team understand the requirements of this permit and their specific responsibilities.
[bookmark: _Toc210027276]5.3	QUALIFIED INSPECTORS
To be considered qualified for conducting inspections under this permit, your inspector must, at a minimum, either:
a.	Have passed the Florida Stormwater Erosion and Sedimentation Control Inspector Training course and assigned a certificate number; or
b.	Hold a current construction inspection certificate, certification, or license from a program that, at a minimum, covers the following:
i.	Principles and practices of erosion and sediment control and pollution prevention practices at construction sites;
ii.	Proper installation and maintenance of erosion and sediment controls and implementation of pollution prevention practices used at construction sites; and
iii.	Inspection procedures, including the proper completion of required reports and documentation, consistent with the requirements of Part 3.
[bookmark: _Toc210027277]6	STORMWATER POLLUTION PREVENTION PLAN (SWPPP)
You must complete the SWPPP prior to submitting the NOI. You must implement the SWPPP upon commencement of construction activities. 
The SWPPP shall document how you will implement the permit requirements.
You must keep the SWPPP and all associated records for three years from the date that the NOT has been submitted or coverage expires.
In accordance with Rule 62-621.260, F.A.C. keep a copy of your SWPPP on-site or at an easily accessible location so that it is available to the Department at the time of an inspection or upon request, including digital/electronic copies or recordkeeping systems.
[bookmark: _Toc210027279]6.1	SWPPP CONTENT
6.1.1	Identification of Operator and Contractors/ Subcontractors and SWPPP Certification. All contractors and subcontractors that are acting under your direction shall be identified in the SWPPP and sign a copy of the following certification statement before conducting any construction activities at the site. The certifications must have the name and title of the person signing the certification, the signature date, and the name, address, and telephone number of the contracting firm. All signed certifications must be included in the SWPPP.
“I certify under penalty of law that I understand, and shall comply with, the terms and conditions of the NPDES Construction Generic Permit.”
6.1.3	Identification of the Stormwater Team. List by name or position the members of the stormwater team (Part 5.1); include their individual responsibilities in implementing the SWPPP. Include documentation or verification (e.g. certificate number) that inspectors are qualified inspectors (Part 5.3).
6.1.4	Description of the Site and Construction Activities
a.	Describe the nature of the construction activities. Include a description of off-site construction support activity, if applicable.
b.	Estimate the total area of the site and total area of planned earth-disturbing areas to the nearest quarter acre;
c.	List and describe all pollutant-generating activities on the site; 
d.	Describe the projected sequence and timetable for the following:
i.	Commencement of construction activities, including land clearing, grubbing, grading, cut and fill, excavating, demolition activities, dewatering operations, final grading, and creation of soil and material stockpiles;
ii.	Temporary or permanent cessation of construction activities in each portion of the site; and
iii.	Final or temporary stabilization of exposed soil for each portion of the site.
6.Description of Stormwater Controls.
a.	Describe the specific controls to be implemented to meet erosion and sediment control requirements, pollution prevention requirements, and dewatering requirements (if applicable), and the projected timeline for installation and/or implementation (Part 2).
b.	Stormwater management systems (e.g., stormwater detention or retention systems) if installed to control pollutants in stormwater discharges during construction;
c.	Spill prevention and response procedures. 
i.	Procedures for stopping, containing, and cleaning up spills, leaks, and other releases associated with the construction site operations; and
ii.	Procedures for notification of appropriate personnel, emergency response and regulatory agencies where a leak, spill, or other release containing a hazardous substance or oil in an amount equal to or in excess of a reportable quantity.
d.	Waste management procedures. Describe the procedures for handling, storing, and disposing of wastes generated at your site consistent with applicable federal or state requirements, including clearing and demolition debris, sediment removed from the site, construction and solid waste, hazardous or toxic waste, and sanitary waste. 
6.1.6	Procedures for Inspections and Maintenance. Include a description of:
a.	Routine maintenance activities and schedules that will be followed to keep BMPs in effective operating condition;
b.	Inspection checklists or other forms that will be used; and
c.	The location of the rain gauge or the identification of the source of rainfall data;
6.1.7	Discharges from Dewatering (if applicable). Include documentation that the dewatering site is not contaminated.
6.1.8	Description of Turbidity Benchmark Monitoring from Dewatering Discharges (if applicable). Describe the procedures you will follow to collect samples, including: 
a. 	Personnel (name(s) or position(s)) that will conduct sampling, 
b. 	Sampling locations, 
c. 	The specific type of turbidity meter you will use for monitoring, as well as a reference to any manuals or manufacturer instructions, and 
d. 	Procedures for documenting monitoring results and weekly averages. 
6.1.9	Site Map. Include a legible site map(s) showing the following features of the site:
a.	Boundaries of the property. 
b.	Locations where construction activities will occur, including: 
i.	Earth-disturbing activities and demolition; note any phasing;
ii.	Approximate slopes and drainage patterns before and after major grading activities;
iii.	Where soil or other construction materials will be stockpiled;
iv.	Any water crossings;
v.	Designated ingress/egress points onto/from paved roads;
vi.	Where structures and other impervious surfaces are planned for construction.
c.	Location and name of receiving surface waters and MS4s.
d.	Points of discharge from the site, including discharges from sheet flow.
e.	Locations of dewatering operations and where turbidity benchmark monitoring will occur, if applicable to your site.
f.	Location of potential pollutant-generating activities and storage areas;
g.	Designated areas where non-pollutant-generating construction wastes will be stored (e.g. scrap wood and metal); and
h.	Locations of stormwater controls (including natural buffer areas), areas which will not be disturbed, and areas where stabilization measures are expected to occur.
6.2	UPDATES TO THE SWPPP
The SWPPP must be kept up-to-date throughout the period of permit coverage; updates to the SWPPP must be signed and dated by the responsible authority or a duly authorized representative; the SWPPP must reflect any changes to the required content within seven days of making or identifying the change; superseded sections/portions of the SWPPP must be kept as attachments to the original plan.
	You must maintain records showing the dates of all SWPPP updates. The records must include a brief summary of all changes.
	If there are multiple contractors/subcontractors covered under this permit, you must immediately notify those that may be impacted by the change to the SWPPP.
[bookmark: _Toc210027281]7	TERMINATING PERMIT COVERAGE
You must submit to DEP a complete and accurate Notice of Termination which certifies that you have met the conditions for terminating coverage. 
Until coverage under this permit is terminated, you must comply with all conditions of the permit.
[bookmark: _Toc210027282]7.1	CONDITIONS FOR TERMINATING CGP COVERAGE
You may only terminate CGP coverage if you have met either of the following conditions:
7.1.1	You have completed all construction activities covered by this permit, all construction activity discharges authorized by this permit have ceased, and you have met all of the following conditions:
a.	For all areas that (1) were disturbed during construction, (2) are not covered by permanent structures, and (3) over which you had control during the construction activities, you have achieved final stabilization.
b.	You have removed or properly disposed of all construction materials, waste and waste handling devices;
c.	You have removed all temporary stormwater controls that were installed and maintained during construction; and
d.	 You have documented conditions a. through c. of this part in a final inspection report.
7.1.2	You no longer operate the construction activity. The new operator will need to develop a SWPPP and submit an NOI and processing fee before construction activities begin or resume. If at any time after you suspend construction activities, you determine that the site will not resume activities during the term of your permit coverage, you must meet the conditions in 7.1.1 and submit a NOT.
7.1.3	Coverage under an alternative NPDES permit has been obtained.
7.2	ADMINISTRATIVE PROCESS FOR TERMINATING COVERAGE
7.2.1	Submitting the Notice of Termination. Submit DEP Form 62-621.300(4)(c), F.A.C. electronically through the DEP electronic submission portal. The responsible authority or a duly authorized representative of the operator must sign the NOT.
7.2.2	Deadline for Submitting The NOT. You must submit a completed NOT within 2 calendar days after meeting any one of the conditions in Part 7.1.
7.2.3	Effective Date of Termination of Coverage
The Department will send you an acknowledgment letter with the date of termination. If your project discharged stormwater to a permitted MS4, you must send a copy of the NOT or the acknowledgement letter within seven calendar days of receipt to the operator of the MS4.
[bookmark: _Toc210027283]8.	GENERAL CONDITIONS. 
[bookmark: _Toc210027284]All general conditions in subsections 62-621.250(1)-(5), F.A.C., are adopted herein by reference. Additionally, general conditions in subsections 62-620.610(1)-(5), (7), (9), (10), (17) and (18), F.A.C., are adopted herein by reference.
[bookmark: _Toc210027285]9.	DEFINITIONS
“Commencement of Construction Activities”
Means the initial disturbance of soil associated with clearing, grading, or excavating activities or other construction activities.
“Common Plan of Development or Sale”
A single plan of development or sale for a site where one or more separate and distinct construction activities are occurring on one or more schedules by one or more contractors. This may include:
· Phased projects and projects with multiple lots, even if the separate phases or lots will be constructed under separate contract or by separate owners (e.g. development where lots are sold to separate builders).
· Projects in a contiguous area that may be unrelated but still under the same contract, such as construction of a building extension and a new parking lot at the same facility.
· Linear projects such as roads, pipelines, or utilities. 
[bookmark: _Hlk195625684]“Construction Activities”
The act or process of developing or improving land through earth-disturbing activities that could lead to the generation of pollutants, including clearing, grading, excavation, demolition and renovation activity.
“Construction Support Activity”
A construction-related activity that specifically supports the construction activity and involves earth disturbance or pollutant-generating activities of its own, and can include activities associated with concrete or asphalt batch plants, equipment staging yards, materials storage/stockpiling areas, excavated material disposal areas, and borrow areas.
“Earth-Disturbing Activity”
Actions taken to alter the existing vegetation and/or underlying soil of a site, such as clearing, grading, site preparation (e.g., excavating, grubbing, cutting, and filling), soil compaction, and movement and stockpiling of topsoil.
“Final Stabilization”
All soil disturbing activities at the site have been completed, and that a uniform (e.g., evenly distributed, without large bare areas) perennial vegetative cover with a density of at least 70% for all unpaved areas and areas not covered by permanent structures has been established or equivalent permanent stabilization measures (e.g., geotextiles) have been employed.
“Operator”
The business, firm, contractor, public organization, person or other legal entity that owns or operates the construction activity and that has authority to exercise operational control over the construction site, activities at the project, and the Stormwater Pollution Prevention Plan (SWPPP), to ensure compliance with the terms and conditions of this permit.
“Sediment-Related Parameter”
For the purposes of this permit, means a pollutant parameter that is closely related to sediment such as turbidity, total suspended solids (TSS), total suspended sediment, transparency, sedimentation, and siltation.
“Storm Event”
A rainfall event that results in a measurable amount of rain. A storm event is defined as a separate event when there is at least four hours of no rain between periods of rainfall.
“Temporary Stabilization”
A condition where exposed soils or disturbed areas are provided a temporary vegetative and/or non-vegetative protective cover to prevent erosion and sediment loss. Temporary stabilization may include temporary seeding, geotextiles, mulches, and other techniques to reduce or eliminate erosion until either final stabilization can be achieved or until further construction activities take place to re-disturb this area.
“Working Day”
Any day on which normal business operations are conducted.
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