## Section C.5: Evaluation of Exposure Routes when Using Non-Recorded ICs

Note that when using a non-recorded IC, such as a local ordinance, governmental control, or MOU to prevent exposure to contaminated groundwater[[1]](#footnote-2) all potential exposure routes should be considered including the possibility of irrigation wells, possibility of construction or utility worker exposure to groundwater, and possibility of new stormwater features that may affect groundwater flow. The potential that some other exposure routes may exist does not prevent the use of local ordinances or governmental controls but may require a layering of multiple controls.

1. ## If applicable, contaminated soil.

   [↑](#footnote-ref-2)