# TIMELINE OF ACTIVITIES

**Pasco County Fire Rescue Training Facility**

|  |  |  |  |
| --- | --- | --- | --- |
| **DATE** | **ACTIONS** | **Program or Agency Involved** | **NOTES** |
| **1/30/19** | Facility outreach conducted. | DEP | DEP contacted the Fire Chief.DEP site number: ERIC\_7395. |
| **2/19/19** | Conducted general visit with facility leadership. | DEP | DEP staff performed a reconnaissance of facility and spoke with facility leadership to identify areas of foam usage. |
| **2/21/19** | Sample Collection at Pasco Fire Rescue Training Facility. | DEP | Water and soil samples collected. |
| **3/19/19** | Certified Pasco County Sampling Results Received. | DEP Central Laboratory | Concentrations of perfluorooctanoateacid (PFOA) and perfluorooctanesulfonic acid (PFOS) has been detected above the Health Advisory Level (HAL).DEP will work with Pasco County on the completion of the assessment and development of a cleanup plan to remove or contain the contamination to prevent environmental impact and human exposure. |
| **3/20/19** | Results shared with Pasco County and DOH. | DEP | DOH has been directed to develop and implement a community sampling plan. |
| **3/29/19** | Letter provided to Pasco County | DEP Southwest District | DEP provided a letter to Pasco County indicating that they may be responsible for further assessment and remediation. |
| **5/16/19** | DEP Central Laboratory certified DOH private supply well results | DOH | DWASTEWELL-2019-05-03-05. Ten supply well results. No PFOA/PFOS HAL exceedances. |
| **5/16/19** | Ten private wells have been sampled by DOH within ½ miles of facility. No groundwater exceedances above the HAL. | DOH | DOH completed potable well sampling. No HAL exceedances. |
| **7/3/19** | DEP Central Laboratory certified DOH private supply well results | DOH | DWASTEWELL-2019-06-25-01. Three supply well results. No PFOA/PFOS HAL exceedances. |
| **7/5/19** | DEP Central Laboratory certified DOH private supply well results | DOH | DWASTEWELL-2019-06-25-01. Five supply well results. No PFOA/PFOS HAL exceedances. |
| **9/2/19** | Pasco County contracted Cardno to conduct sampling | DEP | Cardno will conduct soil and groundwater sampling. |
| **9/19-7/22** | Cardno installed monitor wells and conducted groundwater and soil sampling | DEP | To date they have installed 9 surficial monitoring wells and 5 Floridan monitoring wells. |
| **9/19-7/22** | Cardno sampling results received  | DEP Central Laboratory | Concentrations of perfluorooctanoateacid (PFOA) and perfluorooctanesulfonic acid (PFOS) has been detected above the Health Advisory Level (HAL).Surface groundwater contamination at MW-4, MW-5, and Floridan well MW-9D. These wells are just south or east of the original burn tower. |
| **06-26-2023** | Aptim Issues GMR based on March 2023 groundwater sampling event | DEP-Aptim | MW-4, MW-5, and Floridan well MW-9D exceed PGCTL for PFOA/PFOS. Aptim recommends the installation of additional monitor wells to delineate  |
| **08-21-2024** | SIS issues APTIM Task to install monitor wells and collect groundwater samples | DEP-APTIM |  |
| **11-20-2024** | APTIM notifies SIS of site access difficulties on offsite properties. SIS is unable to gather site access as well. Decision to move wells to Pasco County ROW is made at the end of the year | DEP-APTIM |  |